**Specs 946 Emporio Armani**

|  |  |
| --- | --- |
| **Displacement**  | **125 CC, 4 Stroke** |
| **Maximum power**  | 8.5 Kw @ 8750 Rpm |
|  | 9.6 Nm @ 7750 Rpm |
| **Cooling**  | Air |
| **Supply**  | Electronic Fuel Injection |
| **Front suspension**  | Single link arm with coil spring and dual-action hydraulic shock absorber |
| **Rear Suspension**  | Coil spring with adjustable preload (4 settings) and with dual action hydraulic mono shock with progressive lever system |
| **Front brake**  | Disc 220m |
| **Rear brake**  | Disc 220m |
| **Front tyre**  | 120/70-12” |
| **Rear tyre**  | 130/70-12” |
| **Fuel tank**  | 8,5 Litres |

**Specs Vespa 70th Anniversary Edition**

|  |  |
| --- | --- |
| **Displacement**  | **150 CC, 4 Stroke** |
| **Maximum power**  | 8,5kw @ 7.000 rpm |
| **Maximum torque** | 11,5 Nm @ 5.500 rpm |
| **Cooling**  | Air |
| **Supply**  | Carburetor |
| **Front suspension**  | Aircraft derived single side arm Front Suspension with Anti-Dive characteristics |
| **Rear Suspension**  | Dual-Effect Hydraulic Shock Absorber |
| **Front brake**  | Disc Brake: 200 mm Ventilated |
| **Rear brake**  | 140 mm Rear Drum Brake diameter |
| **Front tyre**  | Tubeless 110/70-11” |
| **Rear tyre**  | Tubeless 120/70-10’’ |